PRESS PUSH START BUTTON



STEPPER MOTOR WILL GO TO FIND THE LIMIT SWITCH AND STOP AT 0,0,0



IR SENSOR ON/OFF?

NO



LED ON

BARCODE SCANNER READ DATA



STEPPER MOTOR MOVING

ARDUINO READ DATA?

SEND DATA TO ARDUINO

NO

YES